|  |  |  |
| --- | --- | --- |
| Image | File name | Caption |
|  | RichardBrink\_Glasgelaender\_01 | Richard Brink has added glass systems to its product portfolio, and now also offers products such as tailor-made glass balustrades.Photo: Richard Brink GmbH & Co. KG |
|  | RichardBrink\_Glasgelaender\_02 | The system consists of stainless-steel posts with glass supports and retaining plates as well as glass panels made from laminated safety glass.Photo: Richard Brink GmbH & Co. KG |
|  | RichardBrink\_Glasgelaender\_03 | The maximum distances between the stainless-steel posts are specified based on the chosen height to guarantee the required stability of the balustrades.Photo: Richard Brink GmbH & Co. KG |
|  | RichardBrink\_Glasgelaender\_04 | The balustrades are firmly affixed using retaining plates at the bottom end of the posts. Photo: Richard Brink GmbH & Co. KG |
|  | RichardBrink\_Glasgelaender\_05 | For the corner connections, the metal products manufacturer provides posts that are able to hold glass panels to either side at a right angle. This maintains the rectangular shape of the balustrade when viewing the solution from the outside.Photo: Richard Brink GmbH & Co. KG |
|  | RichardBrink\_Glasgelaender\_06 | The maximum projection of the systems is 210mm from the outer edge of the post to the fixing point of the retaining plate.Photo: Richard Brink GmbH & Co. KG |
|  | RichardBrink\_Glasgelaender\_07 | Both round and square handrails are available in addition to the stainless-steel end profiles depicted here.Photo: Richard Brink GmbH & Co. KG |